RouterStats History
===================

2.5d	04 Oct	Increased Rx-Sync maximum to 20,000.

2.5c	25 Sep  Added facility to show Login password in plain text to assist when having Login problems.
		Added facility to e-mail IP address if it changes (Netgear DG834(G) only).
		Optional "Mail" icon to notify when an e-mail has been sent.
		Option to open e-mail clent.

2.5b	24 Sep  Added facility to change graph drawing colour when the router doesn't respond. This will
		 allow "genuine" zero values to be distinguished from the router not responding.

2.5a	21 Sep  Fixed bug causing main window to grab focus and move in front of the configuration window.
		Fixed bug causing RouterStats to grab focus from other applications when "closed-to-systray".

		More work to the Login routines - added more error messages to assist finding login failures. 

2.5	19 Sep  Added checkboxes to overlay current Rx-Sync and Rx-Noise values to captured graphs (in addition 
                  to IP address).

		Added prompt for y-axis labels when marking user-defined graphs for "training".

		Moved telnet terminal window onto its own Telnet Tab.

		Removed default login password as this was causing confusion to first-time users.

		A few people seem to have a problem initially getting RouterStats to connect with the router so
		  I've spent some time trying to improve the login routines.

		The success of Telnet seems very variable and seems to depend on factors such as the speed of the
		computer and the ethernet hardware. There's no "handshaking" as such with Telnet so it can be difficult
		to know how the system is performing. I've taken the opportunity to try a few new techniques which
		might improve reliability.

		This is the first version which has had some limited testing with Windows Vista RC1 which seems to place
		higher demands on system hardware. I've included a few notes on using RouterStats with Vista in the
		helpfile.

2.4	10 Sep	Fixed bug causing 'Get Page' button to retrieve the wrong page!

2.3b	04 Sep	Added Telnet facility (Netgear DG834(G) only) to determine if ADSL MAX has Interleaving
		  'On' or 'Off'.

2.3a	03 Sep  Ongoing bug fix with negative Telnet Rx figure. (One occasion when a bad BT line would be
                  useful!)
		Router's Log now automatically scrolls to most recent entry.

2.3	02 Sep	Added Toolbar button to display the router's internal log. NETGEAR DG834(G) only.
		Bug Fix: Adjusted Telnet Rx Noise retrieval code to allow for router error.

2.2b	20 Aug	Added e-mail on alarm facility.

2.2a	20 Aug	Reworked code to try to correct Netgear's problem with negative dB values.

2.2	18 Aug	Added e-mail facility to e-mail a daily Log and the Rx Noise and Rx Sync Speed graphs.

2.1a	16 Aug	Added facility to start a new log each day.

2.0	13 Aug  Added facility to set number of points plotted per page.
		Add facility to expand and restore time axis.
		Fixed bug which caused unselected graphs to be captured if marked for scheduled capture.

1.9g	01 Aug	Added 'Start minimized' checkbox.

1.9f	15 Jul	Logout (if selected) added to application's Close routine.

1.9e	13 Jul	Fixed bug causing Tx Noise graph to always return 0.

1.9d	13 Jul	Minor bug fixes.
		Improved login procedure.

1.9c	11 Jul	Added facility to attempt to work with routers which have decimal and thousands
		  separators "reversed" by UK standards.
		Graphs can now be selected via menu item for adding to Log or not.
		Juggled with positions of "mark" buttons to make them correspond with graph's
		  tabs.  Upper tab and upper button = upload. Lower tab and lower button = download.


1.9	08 Jul	Fixed problem with dragging locked graphs causing system error.
		Added capture facilities to Telnet graphs. Scheduled capture is set using
		  a popup 'checkable' menu item.
		Added similar scheduled capture menu item to main graphs for compatibility and
		  convenience. This simply 'mimics' the existing checkboxes.
		Tightened some code which may improve cpu usage. Fixed bug where selected 
		  telnet graphs were being plotted even when Telnet was not selected.


1.8.1	06 Jul	Attempting to find on-going problem where RouterStats returns rubbish
		values under some conditions. Have re-worked http search code.
		IMPORTANT: Delete routerstats.ini and begin with default values.

1.8	06 Jul	Added Tx Sync Speed graph.
		various minor bug fixes.

1.7	03 Jul	Added 2nd User-defined graph.
		Added "Capture Now" to graph popup menus.
		Captured filenames now derived from y-axis lables.
		Date/time of captured filenames can be formatted.
		Fixed bug where viewer file list was not updating.
		Fixed bug preventing Tx Noise graph from scrolling.
		Added keyboard arrow navigation keys in viewer file list.
		Fixed bug preventing temp bitmap being deleted.
		

1.6c	01 Jul	Telnet Rx Sync Graph - y-axis title corrected.
		Log features added:	Date/time can be formatted.
					Values can be saved as CSV or TabSV.
		Tidied up some panel re-sizing problems.

1.6	30 Jun	Added Upstream (Rx) Noise Graph.
		Fixed problem with Sync Alarms ignoring Delay timers.
		Released as full version.

1.5e	28 Jun	Various cosmetic and small fixes.

1.5d	28 Jun	Tx Interleaved FEC and Tx Interlaeved HEC not remembering checkbox.


1.5c	26 Jun	Bug fixes: Cleared StatusBar filename when Log unchecked.
			   Clear StatusBar if IP lookup fails.
			   Fixed problem with 'camera' icons when form resized.

1.5b	25 Jun	Added IP address lookup.(hard coded via INI file)

1.5	??	Various bug fixed that I've forgotten.

1.4	??	Kept 1.3e as stable version and released 1.4 with Alarm facilities.

............................................


1.3e	21 Jun	Modified auto-scaling for user-defined and telnet graphs.

1.3c/d	2- Jun	Added more Telnet facilities.


1.2a	14 Jun	Increased user-defined upper limit to 2,000,000.

1.2	 8 Jun	Improved Login code. Three attempts to Log in to reduce failures.
		Added experimental Telnet window. ONLY for DG834 and DG834G


1.1	 4 Jun	Improved text search code.
		Added router's stats page to main window.

1.0	 2 Jun	First release version.