I've tested this version of RouterStats using a Netgear DG834GT
flashed with the DGTeam firmware 1.01.32.0743

I've no idea (until someone lets me know!) if it will work with
other DGTeam firmware.


Because RouterStats has been designed to access Telnet without
requiring additional login, the DGTeam telnet login has had to
be a bit "brute force" in that RouterStats doesn't wait for the
login and Password prompts as it should.

I've added a delay to the Telnet login process which should be enough.

It can be changed, if desired, in the routerstats.ini file
under the [Telnet] section: DGTeamTimeout=1000   where '1000' is
1000 msec (ie 1 second).  As RouterStats only has to log in to Telnet
once, there's not much to be gained by reducing this delay although,
if your computer/router combination is slow responding to telnet,
you may get more reliable telnet login by increasing the delay (in,
say, 200msec increments).


The Bits/tone graph is disabled because I can't find the command in
the DGTeam firmware and the "Set Target SNR" facility seems to be
wildly inaccurate!


25 August 2008
John.